## **Airrex ADH-100 Portable Dehumidifier – 1.32 gal/h – 120V**

## **Large Capacity Dehumidifier**

**$1,920.00**

# **Airrex AHD-100 Large Capacity Dehumidifier**

The Airrex ADH-100 is a fully portable dehumidifier providing rapid drying and humidity control.

It is used by restoration companies, for building drying, process drying, and general dehumidification.

Features include an efficient rotary compressor, adjustable humidistat, condensate pump, automatic hot gas bypass, and R-410A.

* **Power Supply: 115V 60Hz**
* **Current Consumption (AMPS): 10**
* **Circuit Breaker Size (AMPS): 15**
* **Rated Power Consumption: 1.2**
* **Amp Rating: 1.2**
* **Evaporator Airflow: 400 CFM**
* **Power Cord Length: 10**
* **Operating Conditions: 41-95°F DBT 30-90%RH**
* **NEMA Plug: 5-15**
* **Noise Level: 60 Db**
* **Moisture Removal Max (Gal/h): 1.32**
* **Weight 132 lbs.**
* **19.9″W x 21.8″D x 39.2″H**